{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Links v4"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Links v4","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,0,0,8],[2,0,2,6],[15,0,15,6]]}
["Links, v4.0"]
["Index","Qty","Description","Specs","Value","Package","Ref. Mouser","References"]
["SMT parts"]
["R2, R4, R5, R12, R13, R21",6,"Resistor, 1%",null,51,{"$f":"\"0603\"","v":"0603"},"667-ERJ-3EKF51R0V"]
["R3, R11, R19",3,"Resistor, 1%",null,"1.0k",{"$f":"\"0603\"","v":"0603"},"667-ERJ3-EKF1001V"]
["R15",1,"Resistor, 1%",null,"33k","0603","667-ERJ-3EKF3302V"]
["R6, R7, R8, R9, R10, R14, R16, R17, R18, R20",10,"Resistor, 0.1%, Thin film",null,"100k","0603","667-ERA-3AEB104V"]
["R1",1,"Resistor, 1%",null,"10M","0603","603-RC0603FR-0710ML"]
["C6, C9",2,"Capacitor, ceramic",">= 16V, <= 5%, C0G","10p","0603","81-GRM185C1H100JA01J"]
["C3, C4, C5, C7, C8, C10",6,"Capacitor, ceramic",">= 16V","100n","0603","81-GRM188R71E104JA1J"]
["C1, C2",2,"Capacitor, electrolytic",">= 25V","4.7u","Panasonic A (3mm dia)","647-UWX1E4R7MCL2","Nichicon UWX1E4R7MCL2GB"]
["D1, D2",2,"1N5819HW diode",null,null,"SOD123","621-1N5819HW-F","Diodes Inc 1N5819HW-7-F"]
["IC2, IC4",2,"TL072 dual op-amp",null,null,"TSSOP8","595-TL072CPWR","Texas Instruments TL072CPW"]
["IC1",1,"OPA4171 quad op-amp",null,null,"TSSOP14","595-OPA4171AIPW","Texas Instruments OPA4171AIPW"]
["IC3, IC5",2,"LM321 single op-amp",null,null,"SOT23-5","926-LM321MFX/NOPB","Texas Instruments LM321MFX/NOPB"]
["PTH parts, top side"]
["J1, J2, J3, J4, J5, J6, J7, J8, J9, J10, J11, J12",12,"Vertical jack connector",{"$nulls":4},"PJ-301-M-12"]
["LED1, LED2, LED3",3,"LED, Red/Green, 2 terminals",null,null,"2 terminals","604-WP937EGW","Kingbright WP937EGW"]
[{"$f":"\"- LED1, LED2, LED3\"","v":"- LED1, LED2, LED3"},3,"LED holder, 3mm LED, 10mm height",{"$nulls":4},"LED3-10 Multicomp; Farnell P/N 9555277"]
["PTH parts, bottom side"]
["JP1",1,"2x5 male header, 2.54mm pitch",null,null,null,"649-67996-410HLF"]
["PCB specifications"]
["PCB",null,"19.0 x 108.4 ; 2 layers"]